**Light Up the Green World . LED Downlights Expert 7 Years**

**New LED COB Downlight**



**1: Model No.** TSD0810

**Product Name:** Oblique Square LED Downlight

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **CRI** | **Size(mm)** | **Cutout(mm)** |
| TSD0810-A | 10W | 850lm | Philips Driver | CREE COB | 3000K  4000K  5000K | 24° | RA>80  RA>90 | SQ85\*H110 | L78\*W78 |
| TSD0810-B | 5W | 430lm | SQ85\*H80 | L78\*W78 |

****

**2: Model no. TD062-8F**

**Product name: 60W LED COB Downlight**

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **CRI** | **Size(mm)** | **Cutout(mm)** |
| TD062-8F | 60W | 5100lm | LinKuan Driver | CREE COB | 3000K  4000K  5000K | 60° | RA>80  RA>90 | D233\*H133 | D210mm |

****

**3: Model no. HSTD002-A**

**Product name: Adjustable Spotlight Downlight**

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **CRI** | **Size(mm)** | **Cutout(mm)** |
| HSTD002-A | 7W | 560lm | Philips Driver | CREE COB | 3000K  4000K  5000K | 10° 20° 30° | RA>80  RA>90 | D85\*H90 | D75 |
| HSTD002-B | 10W | 850lm | D85\*H110 | D75 |

**Hot Selling LED COB Downlight**



**4: Model No.** TD051A TD051B TD051D

**LED COB Downlight**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **Power Factor** | **CRI** | **Size(mm)** | **Cutout(mm)** |
| TD051-2.5F | 5W | 400lm | Philips Driver | CREE COB | 3000K  4000K  5000K | 50° | >0.90 | Ra80/90 | ɸ89.7\*H56 | ɸ75 |
| TD051-3F | 9W | 790lm | ɸ110\*H68 | ɸ90 |
| TD051-4F | 15W | 1300lm | ɸ137.5\*H82 | ɸ120 |
| TD051-5F | 20W | 1700lm | ɸ165\*H91 | ɸ140 |
| TD051-6F | 30W | 2600lm | ɸ195\*H107 | ɸ170 |
| TD051-8F | 40W | 3500lm | ɸ235\*H127.5 | ɸ200 |



**5: Model No.** TD053A TD053B TD053C

**IP54 COB Downlight**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **Power Factor** | **CRI** | **Size(mm)** | **Cutout(mm)** |
| TD053-3F | 10W | 850lm | Philips Driver | CREE COB | 3000K  4000K  5000K | 50° | >0.90 | Ra80/90 | ɸ110\*H61 | ɸ95 |
| TD053-4F | 15W | 1300lm | ɸ135\*H69 | ɸ110 |
| TD053-5F | 25W | 2200lm | ɸ160\*H75 | ɸ130 |
| TD053-6F | 40W | 3500lm | ɸ185\*H100 | ɸ165 |
| TD053-8F | 60W | 4800lm | ɸ240\*H120 | ɸ205 |



**6: Model No.** TD033A TD033B TD033C

**IP44 LED Downlight**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **Power Factor** | **CRI** | **Size(mm)** | **Cutout(mm)** |
| TD033-3F | 9W | 750lm | Philips Driver | CREE COB | 3000K  4000K  5000K | 60° | >0.90 | Ra80/90 | ɸ108\*H52 | ɸ95 |
| TD033-4F | 15W | 1300lm | ɸ142\*H65 | ɸ125 |
| TD033-5F | 20W | 1700lm | ɸ158\*H75 | ɸ140 |
| TD033-6F | 25W | 2200lm | ɸ185\*H88 | ɸ170 |
| TD033-8F | 40W | 3500lm | ɸ226\*H108 | ɸ210 |
| TD033-10F | 60W | 5000lm | ɸ282\*H130 | ɸ265 |



**7: Model No.** TD041

**Horn LED Downlight**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **Power Factor** | **CRI** | **Size(mm)** | **Cutout(mm)** |
| TD041-3F | 9W | 750lm | Philips Driver | CREE COB | 3000K  4000K  5000K | 24°60° | >0.90 | Ra80/90 | ɸ105\*H90.5 | ɸ95 |
| TD041-4F | 15W | 1300lm | ɸ139\*H110.5 | ɸ125 |
| TD041-5F | 25W | 2200lm | ɸ162\*H125.5 | ɸ140 |
| TD041-6F | 40W | 3500lm | ɸ185\*H145 | ɸ170 |



|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **Power Factor** | **CRI** | **Size(mm)** | **Cutout(mm)** |
| TD060-4F | 20W | 1800lm | Philips Driver | CREE COB | 3000K  4000K  5000K | 40° | >0.90 | Ra80/90 | ɸ150\*H80 | ɸ130 |
| TD060-6F | 30W | 2700lm | ɸ195\*H100 | ɸ175 |
| TD060-8F | 40W | 3600lm | ɸ220\*H110 | ɸ200 |

**8: Model No.** TD060

**Product Name: LED COB Downlight**

**9: Model No.** TD056

**SMD COB Downlight**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **Power Factor** | **CRI** | **Size(mm)** | **Cutout(mm)** |
| TD056-4F | 12W | 100lm | Philips Driver | SanAnCOB | 3000K  4000K  6000K | 60° | >0.90 | Ra80/90 | ɸ148\*H63 | ɸ125 |
| TD056-6F | 20W | 1600lm | ɸ195\*H63 | ɸ168 |
| TD056-8F | 30W | 2400lm | ɸ230\*H63 | ɸ190 |
| TD056-10F | 30W | 2400lm | ɸ280\*H88 | ɸ195 |



**10: Model No.** TD057

**LED Downlight with Lens (Max: 80W)**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **Power Factor** | **CRI** | **Size(mm)** | **Cutout(mm)** |
| TD057-A | 15W | 1300lm | Philips Driver | CREE | 3000K  4000K  5000K | 24°  38°60° | >0.90 | Ra80/90 | D115\*H80 | D95 |
| TD057-B | 30W | 2500lm | D142\*H101 | D125 |
| TD057-C | 40W | 3300lm | D160\*H133 | D140 |



**11: Model No. TD036A**

**Product Name: SMD COB LED Downlight**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **​Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **Power Factor** | **CRI** | **Size(mm)** | **Cutout(mm)** |
| TD036A-5F | 10W | 850lm | Philips Driver | SMD | 3000K  4000K  6000K | 100° | >0.90 | Ra80 | D145\*H63 | D125 |
| TD036A-6F | 20W | 1700lm | D196\*H63 | D170 |
| TD036A-8F | 30W | 2500lm | D242\*H63 | D210 |

**Adjustable Downlights**



**12: Model No.** ATD001

**Adjustable LED Downlight**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **Power Factor** | **CRI** | **Size(mm)** | **Cutout(mm)** |
| ATD001-A | 10W | 850lm | Philips Driver | CREE  CITIZEN | 3000K  4000K  5000K | 24°  60° | >0.90 | Ra80/90 | D111\*H90 | D80 |
| ATD001-B | 15W | 1300lm | D120\*H105 | D90 |
| ATD001-C | 20W | 1700lm | D142\*H120 | D110 |
| ATD001-D1/D2 | 30W 40W | 2500lm 3400lm | D180\*H130 | D145/D160 |
| ATD001-E1 | 40W | 3400lm | D194\*H135 | D160 |

****

**13: Model No.** ATD002

**Product Name: Eyeball LED Downlight 1 Head**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **Power Factor** | **CRI** | **Size(mm)** | **Cutout(mm)** |
| ATD002-3F | 12W | 1050lm | Philips Driver | CREE | 3000K  4000K  5000K | 15°  24°  40° | >0.90 | Ra80/90 | D115\*H95 | D95 |
| ATD002-4F | 15W | 1300lm | D115\*H105 | D95 |
| ATD002-5F | 20W | 1700lm | D135\*H120 | D120 |
| ATD002-6F | 30W | 2600lm | D135\*H130 | D120 |



****

**14: Model No. ATD002-2**

**Product Name: Eyeball LED Downlight 2 Heads**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **Power Factor** | **CRI** | **Size(mm)** | **Cutout(mm)** |
| ATD002-2-A | 2\*12W | 2\*1000lm | Philips Driver | CREE | 3000K  4000K  5000K | 15°  24°  38° | >0.90 | Ra80/90 | W115\*L210\*H95 | W95\*L190 |
| ATD002-2-B | 2\*20W | 2\*1700lm | W135\*L250\*H120 | W115\*L230 |
| ATD002-2-C | 2\*30W | 2\*2500lm | W135\*L250\*H130 | W115\*L230 |

**360 Degree Rotatable Downlights**

****

**15: Model No.** RADL005

**Product Name:** 360°Rotatable LED Downlight

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **CRI** | **Size(mm)** | **Cutout(mm)** |
| RADL005-A | 3W | 250lm | Philips Driver | CREE COB | 3000K  4000K  5000K | 60° | RA>80  RA>90 | D70\*H30 | D55 |
| RADL005-B | 5W | 400lm | D88\*H33 | D75 |
| RADL005-C | 7W | 600lm | D110\*H35 | D95 |

****

**16: Model No.** SD005-6F

**Product Name:** Double Rings Adjustable Downlight

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **CRI** | **Size(mm)** | **Cutout(mm)** |
| SD005-6F | 30W | 2700lm | Philips Driver | CREE COB | 3000K  4000K  5000K | 24° | RA>80  RA>90 | D165\*H95 | D145 |
| SD005-8F | 40W | 3500lm | D198\*H130 | D165 |

**17: Model No.** SD001

**LED Gimbal Downlight**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **Power Factor** | **CRI** | **Size(mm)** | **Cutout(mm)** |
| SD001-3F | 7W | 550lm | Philips Driver | CREE COB | 3000K  4000K  5000K | 24° | >0.90 | Ra80/90 | ɸ86\*H68 | ɸ70 |
| SD001-4F | 12W | 1000lm | ɸ118\*H65 | ɸ90 |
| SD001-5F | 20W | 1700lm | ɸ140\*H80 | ɸ120 |
| SD001-6F | 30W | 2500lm | ɸ160\*H125 | ɸ145 |




**18: Model No.** SD004

**LED Square Downlight**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **Power Factor** | **CRI** | **Size(mm)** | **Cutout(mm)** |
| SD004A | 30W | 2400lm | Philips Driver | CREE COB | 3000K  4000K  5000K | 12°24°36° | >0.90 | Ra80/90 | SQ175\*H145 | 150\*150 |
| SD004B | 50W | 4000lm | SQ175\*H180 | 150\*150 |
| SD004C | 2\*30W | 2\*2400lm | 175\*325\*H145 | 150\*300 |
| SD004D | 2\*50W | 2\*4000lm | 175\*325\*H180 | 150\*300 |

**LED Downlight Module**

**Model No.** DLM001-A DLM001-B DLM001-C DLM001-D

**19: Model No.** DLM001-E DLM001-F DLM001-C

**Modular Downlight**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **Power Factor** | **CRI** | **Size(mm)** | **Cutout(mm)** |
| DLM001-A | 10W | 850lm | Philips Driver | CREE COB | 3000K  4000K  6000K | 15°24°36° | >0.90 | Ra80/90 | SQ95\*H98 | 85\*85 |
| 15W | 1300lm | SQ95\*H103 |
| DLM001-B | 10W | 850lm | SQ105\*H113 | 95\*95 |
| 15W | 1300lm | SQ105\*H118 |
| DLM001-C | 10W | 850lm | SQ95\*H118 | 85\*85 |
| 15W | 1300lm | SQ95\*H123 |
| DLM001-D | 10W | 850lm | ɸ95\*H98 | ɸ85 |
| 15W | 1300lm | ɸ95\*H103 |
| DLM001-E | 10W | 850lm | ɸ90\*H105 | ɸ80 |
| 15W | 1300lm | ɸ90\*H110 |
| DLM001-F | 10W | 850lm | ɸ85\*H105 | ɸ77 |
| 15W | 1300lm | ɸ85\*H112 |




    

**20: Model No.** DLM002

**Trimless Modular Downlight**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **Power Factor** | **CRI** | **Size(mm)** | **Cutout(mm)** |
| DLM002-A | 5W | 400lm | Philips Driver | CREE COB | 3000K  4000K  6000K | 15°24°38°  55° | >0.90 | Ra80/90 | ɸ91\*H78 | ɸ92 |
| DLM002-B | 10W | 800lm | ɸ91\*H115 |


**LED Linear Downlight**

**21: Model No.** XTD-B

**Trimless Linear Downlight**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **Power Factor** | **CRI** | **Size(mm)** | **Cutout(mm)** |
| XTD-B-01 | 2W\*1 | 150lm | Philips Driver | CREE Osram | 3000K  4000K  5000K | 15°30°45° | >0.90 | Ra80/90 | 35\*35\*H49 | 42\*42 |
| XTD-B-02 | 2W\*2 | 300lm | 65\*35\*H49 | 72\*42 |
| XTD-B-05 | 2W\*5 | 800lm | 138\*35\*H49 | 144\*42 |
| XTD-B-10 | 2W\*10 | 1700lm | 270\*35\*H49 | 277\*42 |
| XTD-B-15 | 2W\*15 | 2500lm | 403\*35\*H49 | 409\*42 |

**22: Model No.** XTD-A

**LED Linear Downlight with Trim**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **Power Factor** | **CRI** | **Size(mm)** | **Cutout(mm)** |
| XTD-A-01 | 2W\*1 | 150lm | Philips Driver | CREE Osram | 3000K  4000K  5000K | 15°30°45° | >0.90 | Ra80/90 | 45\*45\*H49 | 37\*37 |
| XTD-A-02 | 2W\*2 | 300lm | 75\*45\*H49 | 68\*37 |
| XTD-A-05 | 2W\*5 | 800lm | 147\*45\*H49 | 140\*37 |
| XTD-A-10 | 2W\*10 | 1700lm | 280\*45\*H49 | 273\*37 |
| XTD-A-15 | 2W\*15 | 2500lm | 415\*45\*H49 | 405\*37 |

**Surface Mounted LED Downlight**



**23: Model No. SMDL003**

**Product Name: Round Surface Mounted Downlight**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **Power Factor** | **CRI** | **Size(mm)** | **Height(mm)** |
| SMDL003-4F | 9W | 750lm | Philips Driver | CREE | 3000K  4000K  5000K | 24°45° | >0.90 | Ra80/90 | D90 | 90 |
| SMDL003-5F | 15W | 1300lm | D110 | 120 |
| SMDL003-6F | 25W | 1700lm | D130 | 152 |
| SMDL003-8F | 35W | 2500lm | D170 | 185 |

**   **

**23: Model No. SMDL002**

**Product Name: Square Surface Mounted Downlight**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **Power Factor** | **CRI** | **Size(mm)** | **Height(mm)** |
| SMDL002-4F | 9W | 750lm | Philips Driver | CREE | 3000K  4000K  5000K | 24°45° | >0.90 | Ra80/90 | 90\*90 | 90 |
| SMDL002-5F | 20W | 1700lm | 110\*110 | 120 |
| SMDL002-6F | 30W | 2500lm | 130\*130 | 135 |
| SMDL002-8F | 40W | 3300lm | 160\*160 | 165 |

**24: Model No.** SMDL001

**Square Surface Mounted Downlight**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **Power Factor** | **CRI** | **Size(mm)** | **Height(mm)** |
| SMDL001-4F | 10W | 850lm | Philips Driver | CREE | 3000K  4000K  5000K | 24° | >0.90 | Ra80/90 | 80\*80 | 103 |
| SMDL001-5F | 15W | 1300lm | 100\*100 | 112 |
| SMDL001-6F | 20W | 1700lm | 120\*120 | 133 |
| SMDL001-8F | 30W | 2500lm | 150\*150 | 142 |



**25: Model No.** ASMDL002-3F

**Product Name:** Adjustable Surface Mounted LED Downlight

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **CRI** | **Size(mm)** |
| ASMDL002-3F | 10W | 850lm | Philips Driver | CREE COB | 3000K  4000K  5000K | 24° | RA>80  RA>90 | D68\*H198 |


**LED Gimbal Downlight**



**26: Model No.** SD002

**LED Gimbal Downlight**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **Power Factor** | **CRI** | **Size(mm)** | **Cutout(mm)** |
| SD002-2.5F | 7W | 550lm | Philips Driver | CREE COB | 3000K  4000K  5000K | 24° | >0.90 | Ra80/90 | ɸ85\*H78 | ɸ76 |
| SD002-4F | 15W | 1300lm | ɸ130\*H110 | ɸ120 |
| SD002-5F | 30W | 2500lm | ɸ165\*H143 | ɸ155 |
| SD002-6F | 40W | 3500lm | ɸ190\*H155 | ɸ170 |



**27: Model No. SD005**

**Product Name: LED Trunk Downlight**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **Power Factor** | **CRI** | **Size(mm)** | **Cutout(mm)** |
| SD005-2.5F | 10W | 850lm | Philips Driver | CREE | 3000K  4000K  5000K | 24°  38° | >0.90 | Ra80/90 | D90\*H70 | D75 |
| SD005-3F | 15W | 1300lm | D115\*H125 | D100 |
| SD005-4F | 25W | 2200lm | D138\*H120 | D128 |
| SD005-5F | 35W | 2900lm | D165\*H155 | D145 |
| SD005-6F | 40W | 3500lm | D190\*H165 | D175 |

**LED Wall Washer Downlight**

**28: Model No.** HSTD001

**LED Wall Washer Downlight**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **Power Factor** | **CRI** | **Size(mm)** | **Cutout(mm)** |
| HSTD001-A | 10W | 850lm | Philips Driver | CREE | 3000K  4000K  5000K | 24°  38° | >0.90 | Ra80/90 | D90\*H113 | D78 |
| HSTD001-B | 15W | 1300lm | D90\*H134 | D78 |
| HSTD001-C | 20W | 1700lm | D120\*H116 | D100 |
| HSTD001-D | 40W | 3500lm | D160\*H156 | D140 |

**LED Spot Downlight**

****

**29: Model No.** TSD0808

**Oblique Downlight Square**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **Power Factor** | **CRI** | **Size(mm)** | **Cutout(mm)** |
| TSD0808-A | 10W | 800lm | Philips Driver | CREE | 3000K  4000K  5000K | 24° | >0.90 | Ra80/90 | SQ95\*H98 | 80\*80 |
| TSD0808-B | 15W | 1200lm | SQ115\*H120 | 100\*100 |

****

**30: Model No.** TSD0816

**Spot Downlight**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **Power Factor** | **CRI** | **Size(mm)** | **Cutout(mm)** |
| TSD0816-A | 10W | 850lm | Philips Driver | CREE | 3000K  4000K  5000K | 24° | >0.90 | Ra80/90 | SQ75\*H65 | D70 |
| TSD0816-B | 15W | 1300lm | SQ100\*H85 | D90 |
| TSD0816-C | 20W | 1700lm | SQ135\*H110 | D115 |



**31: Model No. TSD0806**

**Product Name: Square Adjustable LED Downlight 10W 15W 20W**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **Power Factor** | **CRI** | **Size(mm)** | **Cutout(mm)** |
| TSD0806-A | 10W | 850lm | Philips Driver | CREE | 3000K 4000K 5000K | 24° | >0.90 | Ra80/90 | SQ85\*H65 | D75 |
| TSD0806-B | 15W | 1300lm | SQ110\*H85 | D95 |
| TSD0806-C | 20W | 1700lm | SQ145\*H100 | D115 |



**32: Model No. TSD0803**

**Product Name: Round LED Spot Downlight**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **Power Factor** | **CRI** | **Size(mm)** | **Cutout(mm)** |
| TSD0803-A | 10W | 850lm | Philips Driver | CREE | 3000K 4000K 5000K | 24° | >0.90 | Ra80/90 | D80\*H90 | D75 |
| TSD0803-B | 15W | 1300lm | D100\*H115 | D90 |
| TSD0803-C | 20W | 1700lm | D135\*H145 | D115 |

**LED Grille Downlights**



**33: Model No.** DD001-1

**LED Grille Light 1 Head**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **Power Factor** | **CRI** | **Size(mm)** | **Cutout(mm)** |
| DD001-1-A | 10W | 850lm | Philips Driver | CREE  CITIZEN | 3000K  4000K  5000K | 24°  60° | >0.90 | Ra80/90 | SQ140\*H144 | 125\*125 |
| DD001-1-B | 15W | 1300lm | SQ160\*H163 | 145\*145 |
| DD001-1-C | 25W | 2200lm | SQ190\*H173 | 170\*170 |
| DD001-1-D | 40W | 3400lm | SQ203\*H188 | 185\*185 |



**34: Model No.** DD001-2

**LED Grille Light 2 Heads**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **Power Factor** | **CRI** | **Size(mm)** | **Cutout(mm)** |
| DD001-2-A | 2\*10W | 2\*850lm | Philips Driver | CREE  CITIZEN | 3000K  4000K  5000K | 24°  60° | >0.90 | Ra80/90 | 260\*140\*H144 | 245\*125 |
| DD001-2-B | 2\*15W | 2\*1300lm | 320\*160\*H163 | 305\*145 |
| DD001-2-C | 2\*25W | 2\*2200lm | 375\*190\*H173 | 355\*170 |
| DD001-2-D | 2\*40W | 2\*3400lm | 405\*203\*H188 | 385\*185 |



**35: Model No.** DD001-3

**LED Grille Light 3 Heads**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **Power Factor** | **CRI** | **Size(mm)** | **Cutout(mm)** |
| DD001-3-A | 3\*10W | 3\*850lm | Philips Driver | CREE  CITIZEN | 3000K  4000K  5000K | 24°  60° | >0.90 | Ra80/90 | 372\*140\*H144 | 360\*125 |
| DD001-3-B | 3\*15W | 3\*1300lm | 462\*160\*H163 | 450\*145 |
| DD001-3-C | 3\*25W | 3\*2200lm | 538\*190\*H173 | 520\*170 |



**36: Model No. GSD1201**

**Product Name: LED Grille Downlight 12W**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model No.** | **Power** | **Lumen(lm)** | **Driver Brand** | **LED Style** | **CCT(K)** | **Beam Angle** | **Power Factor** | **CRI** | **Size(mm)** | **Cutout(mm)** |
| GSD1201-1-A | 1\*12W | 1000lm | Philips Driver | CREE | 3000K  4000K  5000K | 15°  24° | >0.90 | Ra80/90 | 133\*132\*110 | 120\*120 |
| GSD1201-2-A | 2\*12W | 2\*1000lm | 232\*132\*110 | 220\*120 |
| GSD1201-3-A | 3\*12W | 3\*1000lm | 240\*132\*110 | 330\*120 |
| GSD1201-4-A | 4\*12W | 4\*1000lm | 232\*232\*110 | 225\*225 |