**LED Flat Downlight Specification**



|  |  |  |  |
| --- | --- | --- | --- |
| **Model** | TD056-4F | TD056-6F | TD056-8F |
| **LED Light Source** | CREE LED/Citizen LED/SMD5630 |
| **Lamp Watt** | 10-12W | 20W | 30W |
| **Lamp Lumen** | 880lm | 1700lm | 2500lm |
| **Input Voltage** | AC100-240V |
| **Size** | D148\*H63mm | D195\*H63mm | D230\*H63mm |
| **Cut Hole** | D125mm | D168mm | D195mm |
| **Inner Package** | 15\*15\*7cm | 20\*20\*7cm | 23.5\*23.5\*7cm |
| **CRI** | >80 |
| **Beam Angle** | 90°/ 120 ° |
| **CCT** | 3000K,4000K,5000K,6000K |
| **Material** | Die-cast Aluminum+Al Reflector+Clear Glass Cover/Frosted PC Cover |
| **Adjustable** | Not-Adjustable |
| **PF** | >0.90(50/60Hz) |
| **Outlook** | White+Black Heat Sink |
| **Working Temperature** | -20 to 50℃ |
| **IP Rate** | IP44 |
| **Warranty**  | 3 Years |
| **Package** | White Inner Box |